**ADVERTISEMENT FOR BIDS**

Notice is hereby given that sealed bids will be received by the Adams County Board of Supervisors for the purchase, from the lowest and best bidder, One (1) 25-Ton TAG-A-LONG w/Air Ride/Air Lift Front Axle, for the Department of Road Maintenance. Bids must be received by 10:30 A. M., Monday, October 5, 2020 at the County Administration Building, 314 State Street, Natchez, Mississippi.

Specifications for the 25-Ton TAG-A-LONG w/Air Ride/Air Lift Front Axle can be emailed by requesting via [fbell@adamscountyms.gov](mailto:fbell@adamscountyms.gov) or picked up.

Bids submitted with qualifications or exceptions will not be considered.

All bids are to be SEALED, PLAINLY ADDRESSED TO THE ADAMS COUNTY BOARD OF SUPERVISORS, and outside of envelope containing bids should be marked; “BID ON (# Item Bidding On)”.

Bids may be hand delivered to 314 State Street, Natchez, Mississippi or mailed to the Board of Supervisors’ County Administration Building at the just mentioned address.

Bid prices are to be firm and not subject to change during the period specified above.

The Board of Supervisors reserves the right to waiver informalities and to reject any and all bids.

FRANCES BELL

PURCHASE CLERK

601-445-7941 or 601-597-3160

BRANDI LEWIS

CHANCERY CLERK

ADAMS COUNTY, MISSISSIPPI

--------------------------------------------------------------------------------------------

**PUBLICATION DATES: Friday, September 11, 2020**

**Friday, September 18, 2020**

**BID OPENING DATE: Monday, October 5, 2020**

**SPECIFICATIONS FOR 25-TON TAG-A-LONG**

**With Air Ride/Air Lift Front Axle**

**FRAMEWORK:**

Main Frame: 14” I-Beam 30# per ft.

Cross Members: 4” I-Beam 7.7# per ft. w/gussets (pierced thru main frame)

Side Rails: 10” channel 15.3# per ft.

Head Rail: 8”

**UNDERCARRIAGE:**

Three 22,500# oil bath axles

12 ¼” x 7 ½” brakes, all axles

8-hole Budd wheels (12) Unimount

Front axle: 235/75R17.5 16-ply radial tires (4) with air ride/air lift

Rear axles: 235/75R17.5 16-ply radial tires (8) with 9700 Hutch Suspension

Air brakes (Spring/Maxi brakes on rear axle)

**DIMENSIONS:**

Bed Length 31’ including 6’ dove tail

Overall Width 8 ½’ Height 35 ¾” (unloaded)

11’ hydraulically operated folding ramps (self-contained electric/hydraulic)

5’ tongue with locking lid

**MISCELLANEOUS SPECIFICATIONS:**

Adjustable 3” pintle ring, 90,000#

High tensile safety chains

Twin 2-speed jacks

DOT sealed beam lights (LED)

Mud flaps

Protected wiring system

Stake pockets and D-rings along each side

2” hardwood decking

Ramps: 3’ wide each

Color: Industrial Yellow (options available)

Other options available

FOB Natchez, MS