OFFICE OF STATE AID ROAD CONSTRUCTION

MISSISSIPPI DEPARTMENT OF TRANSPORTATION

AND

JACKSON COUNTY BOARD OF SUPERVISORS

SECTION 900

NOTICE TO CONTRACTORS:

Sealed or electronic bids will be received by the Board of Supervisors of Jackson County, Mississippi for the construction of 2.079 miles of Grade, Drain, Base, surfacing & Box Bridges for **I-10 CONNECTOR / MALLET ROAD** being known as Project No. MS 134-030(2)B in Jackson County, Mississippi, **no later than 12:00 p.m. Local Time, June 23, 2021**, at the office of the Clerk of the Board of Supervisors of Jackson County, 2915 Canty Street, Suite R, Pascagoula, MS 39567. All bids so received will be publicly opened and read aloud at **1:00 p.m. Local Time, June 23, 2021**, at the Board of Supervisors Meeting Room, 2915 Canty Street, Pascagoula, MS 39567.

A Pre-Bid Conference will be held at **1:00 p.m. Local Time, June 16, 2021**, at the Board of Supervisors Meeting Room, 2915 Canty Street, Pascagoula, MS 39567. Attendance at the Pre-Bid Conference is **MANDATORY** for all Bidders. Failure to attend the Pre-Bid Conference will disqualify bids from any company not represented by a qualified agent of the company.

PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

 ITEM QUANTITY UNIT

ROADWAY ITEMS:

MOBILIZATION LUMP SUM LS

CLEARING AND GRUBBING LUMP SUM LS

REMOVAL OF OBSTRUCTIONS LUMP SUM LS

REMOVAL OF DRAINAGE STRUCTURES 8.00 UN

REMOVAL OF TRAFFIC SIGNAL POLE AND APPURTENANCES 2.00 UN

REMOVAL OF TRAFFIC SIGNAL POLE FOUNDATION

(2’ BELOW FINISHED GRADE) 2.00 UN

REMOVAL OF CONCRETE CURB AND CURB AND GUTTER 1,482.00 LF

REMOVAL OF FENCING, ALL TYPES 800.00 LF

REMOVAL OF ASPHALT PAVEMENTS, ALL DEPTHS 10,316.00 SY

REMOVAL OF PAVED DRIVEWAYS AND SIDEWALKS, ALL DEPTHS 1,801.00 SY

REMOVAL OF PIPE (ALL TYPES AND SIZES) 4,420.00 LF

UNCLASSIFIED EXCAVATION (FM) 14,267.00 CY

BORROW EXCAVATION (FME) (CONTRACTOR FURNISHED) (CLASS B-3) 45,618.00 CY

BORROW EXCAVATION (FME) (CONTRACTOR FURNISHED) (CLASS B-5) 16,013.00 CY

EXCESS EXCAVATION (FM) 53,639.00 CY

GEOTEXTILE FABRIC STABILIZATION (TYPE VII) (WOVEN-AOS 0.15-0.21) 47,390.00 SY

TEMPORARY STREAM DIVERSION 2.00 EA

CRUSHED STONE SIZE 610, (FM) 8,384.00 CY

SIZE II STABILIZER AGGREGATE, COARSE 435.00 CY

SECTION 900

PROJECT NO. MS 134-030(2)B

JACKSON COUNTY

 ITEM QUANTITY UNIT

SIZE III STABILIZER AGGREGATE, COARSE 139.00 CY

HOT MIX ASPHALT, MT 9.5-MM MIXTURE 5,386.00 TON

HOT MIX ASPHALT, MT 12.5-MM MIXTURE 3,495.00 TON

HOT MIX ASPHALT, MT 19-MM MIXTURE 6,991.00 TON

HOT MIX ASPHALT, MT, LEVELING, 12.5MM MIXTURE 2,798.00 TON

COLD MILLING OF BITUMINOUS PAVEMENT, ALL DEPTHS 23,122.00 SY

ASPHALT FOR TACK COAT 11,870.00 GAL

CLASS B STRUCTURAL CONCRETE 189.00 CY

CLASS B STRUCTURAL CONCRETE, MINOR STRUCTURES 411.00 CY

REINFORCING STEEL 46,782.00 LB

18” REINFORCED CONCRETE PIPE, CLASS III 7,329.00 LF

24” REINFORCED CONCRETE PIPE, CLASS III 601.00 LF

18” REINFORCED CONCRETE PIPE, END SECTION 4.00 EA

22” X 13” REINFORCED CONCRETE ARCH PIPE, CLASS III 16.00 LF

29” X 18” REINFORCED CONCRETE ARCH PIPE, CLASS III 341.00 LF

36” X 23” REINFORCED CONCRETE ARCH PIPE, CLASS III 177.00 LF

44” X 27” REINFORCED CONCRETE ARCH PIPE, CLASS III 286.00 LF

51” X 31” REINFORCED CONCRETE ARCH PIPE, CLASS III 186.00 LF

65” X 40” REINFORCED CONCRETE ARCH PIPE, CLASS III 101.00 LF

22” X 13” REINFORCED CONCRETE ARCH PIPE, END SECTION 1.00 EA

29” X 18” REINFORCED CONCRETE ARCH PIPE, END SECTION 1.00 EA

36” X 23” REINFORCED CONCRETE ARCH PIPE, END SECTION 5.00 EA

44” X 27” REINFORCED CONCRETE ARCH PIPE, END SECTION 4.00 EA

51” X 31” REINFORCED CONCRETE ARCH PIPE, END SECTION 4.00 EA

65” X 40” REINFORCED CONCRETE ARCH PIPE, END SECTION 2.00 EA

CASTINGS 5,966.00 LB

GRATINGS 681.00 LB

ROADWAY CONSTRUCTION SURVEYING LUMP SUM LS

48” CLASS I CHAIN LINK FENCE 180.00 LF

CONCRETE SIDEWALK 10,271.00 SY

CONCRETE DRIVEWAY, WITHOUT REINFORCEMENT 2,775.00 SY

DETECTABLE WARNING PANELS 224.00 SF

CONCRETE CURB, HEADER 480.00 LF

COMBINATION CONCRETE CURB AND GUTTER, TYPE 1 MODIFIED 27,899.00 LF

COMBINATION CONCRETE CURB AND GUTTER, TYPE 2 297.00 LF

ADJUSTMENT OF CASTINGS, GRATINGS AND UTILITY APPURTENANCES LUMP SUM LS

CONCRETE ISLAND PAVEMENT 2,024.00 SY

RIGHT OF WAY MARKERS (TYPE II) 60.00 EA

MAINTENANCE OF TRAFFIC LUMP SUM LS

ADDITIONAL CONSTRUCTION SIGNS 0.00 SF

4” WIDE TEMPORARY TRAFFIC STRIPE 35,000.00 LF

6” WIDE THERMOPLASTIC TRAFFIC STRIPE (SKIP WHITE) (90 MILS) 3.080 MI

6” WIDE THERMOPLASTIC EDGE STRIPE (CONTINUOUS WHITE) (60 MILS) 3.470 MI

SECTION 900

PROJECT NO. MS 134-030(2)B

JACKSON COUNTY

 ITEM QUANTITY UNIT

6” WIDE THERMOPLASTIC TRAFFIC STRIPE

 (SKIP YELLOW) (60 MILS) 0.090 MI

6” WIDE THERMOPLASTIC TRAFFIC STRIPE

(CONTINUOUS YELLOW) (90 MILS) 1,384.00 LF

6” WIDE THERMOPLASTIC EDGE STRIPE

 (CONTINUOUS YELLOW) (60 MILS) 3.030 MI

THERMOPLASTIC DETAIL STRIPE (4” EQUIVALENT LENGTH)

 (WHITE) (90 MILS) 3,495.00 LF

THERMOPLASTIC DETAIL STRIPE (4” EQUIVALENT LENGTH)

 (YELLOW) (90 MILS) 1,619.00 LF

THERMOPLASTIC LEGEND (WHITE) (120 MILS) 507.00 LF

THERMOPLASTIC LEGEND (WHITE) (120 MILS) 1,578.00 SF

ENGINEER’S FIELD OFFICE BUILDING, TYPE 2 1.00 EA

RED CLEAR REFLECTIVE RAISED MARKERS 481.00 EA

TWO-WAY YELLOW REFLECTIVE RAISED MARKERS 132.00 EA

STANDARD ROADSIDE SIGNS, LESS THAN 10 SQ. FT. 212.00 SF

STEEL U-SECTION POST, 3-3.5 LB./LF 345.00 LF

EROSION CONTROL ITEMS:

TEMPORARY GRASSING 9.80 AC

SOLID SODDING, CENTIPEED 15,404.00 SY

HYDROSEEDING 4.50 AC

EROSION CONTROL FABRIC 3,493.00 SY

TEMPORARY SILT FENCE, TYPE II 15,598.00 LF

WATTLES, 20” 2,040.00 LF

GROUTED RIPRAP 185.00 SY

GEOTEXTILE UNDER RIPRAP (TYPE V) 200.00 SY

BRIDGE ITEMS:

BOX BRIDGE CONCRETE, CLASS BB 235.00 CY

REINFORCEMENT 30,652.00 LB

TRAFFIC SIGNAL ITEMS:

SOLID STATE TRAFFIC SIGNAL CABINET ASSEMBLY, TYPE III CABINET,

TYPE I CONTROLLER 1.00 EA

POWER SERVICE PEDESTAL 1.00 EA

TRAFFIC SIGNAL EQUIPMENT POLE, TYPE II(L), 30’ SHAFT, 45’ ARM 1.00 EA

TRAFFIC SIGNAL EQUIPMENT POLE, TYPE II(L), 30’ SHAFT, 50’ ARM 1.00 EA

SECTION 900

PROJECT NO. MS134-0030(2)B

JACKSON COUNTY

 ITEM QUANTITY UNIT

TRAFFIC SIGNAL EQUIPMENT POLE, TYPE II, 17’ SHAFT, 45’ ARM 1.00 EA

TRAFFIC SIGNAL EQUIPMENT POLE, TYPE II, 17’ SHAFT, 65’ ARM 1.00 EA

POLE FOUNDATION, CLASS “DS” CONCRETE 16.00 CY

SLIP CASING, 36” DIAMETER 60.00 LF

TRAFFIC SIGNAL HEADS, TYPE 1 8.00 EA

TRAFFIC SIGNAL HEADS, TYPE 2 3.00 EA

TRAFFIC SIGNAL HEADS, TYPE 2FYA 2.00 EA

TRAFFIC SIGNAL HEADS, TYPE 6 6.00 EA

ELECTRIC CABLE, UNDERGROUND IN CONDUIT, IMSA 20-1, AWG 10,

 2 CONDUCTOR 250.00 LF

ELECTRIC CABLE, UNDERGROUND IN CONDUIT, IMSA 20-1, AWG 14,

 5 CONDUCTOR 350.00 LF

ELECTRIC CABLE, UNDERGROUND IN CONDUIT, IMSA 20-1, AWG 14,

 8 CONDUCTOR 450.00 LF

ELECTRIC CABLE, UNDERGROUND IN CONDUIT, IMSA 20-1, AWG 6,

 3 CONDUCTOR 40.00 LF

ELECTRIC CABLE, AERIAL SUPPORTED IN CONDUIT, IMSA 20-1, AWG 10,

 2 CONDUCTOR 76.00 LF

ELECTRIC CABLE, AERIAL SUPPORTED IN CONDUIT, IMSA 20-1, AWG 14,

 5 CONDUCTOR 72.00 LF

ELECTRIC CABLE, AERIAL SUPPORTED IN CONDUIT, IMSA 20-1, AWG 14,

 8 CONDUCTOR 250.00 LF

PULL BOX ENCLOSURE, TYPE 2 4.00 EA

PULL BOX ENCLOSURE, TYPE 3 1.00 EA

TRAFFIC SIGNAL CONDUIT, UNDERGROUND, TYPE 4, 2” 35.00 LF

TRAFFIC SIGNAL CONDUIT, UNDERGROUND, TYPE 4, 3” 50.00 LF

TRAFFIC SIGNAL CONDUIT, UNDERGROUND DRILLED OR JACKED,

ROLLED PIPE, 3” 300.00 LF

VIDEO VEHICLE DETECTION SENSOR, TYPE 1A 2.00 EA

VIDEO VEHICLE DETECTION CABLE 350.00 LF

MULTI-SENSOR VEHICLE DETECTION SENSOR 2.00 EA

MULTI-SENSOR VEHICLE DETECTION CABLE 350.00 LF

ACCESSIBLE PEDESTRIAN DETECTION ASSEMBLY 6.00 EA

STREET NAME SIGN 27.00 SF

NOTICE TO CONTRACTORS: PROJECT NO. MS 134-030(2)B

JACKSON COUNTY

CONTRACT TIME: 232 Working Days

BASIS OF AWARD

The award, if made, will be made to the lowest qualified bidder which attended the Pre-Bid Conference on the basis of published quantities.

Any contract awarded under this Advertisement for Bids may be paid for in whole or in part with grant funding from the Department of the Treasury and the Mississippi Department of Environmental Quality under the Resources and Ecosystems Sustainability, Tourist Opportunities, and Revived Economies of the Gulf Coast Sates Act of 2012 (RESTORE Act). Any contract resulting from this solicitation will be subject to the terms and conditions of said funding award, the RESTORE Act Financial Assistance Standard Terms and Conditions and Program-Specific Terms and Conditions, the Standard Sub-Award Terms and Conditions, the RESTORE Act, 33 U. S. C. 1321(t), Treasury Regulations 31 C. F. R. § 34 et seq., including 31 C. F. R. §§ 34, Subpart D, all applicable terms and conditions in 2 C. F. R. Part 200 (including Appendix II to Part 200), and all other OMB circulars, executive orders or other federal laws or regulations, as applicable. The Mississippi Department of Environmental Quality, the United States, or any of its departments, agencies or employees is not and will not be a party to this Invitation for Bids or any resulting contract.

The attention of the BIDDER is directed to the State and Federal laws governing selection of and employment of labor.

The Board of Supervisors herby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprise will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color, or national origin in consideration for an award.

Minority and women’s business enterprises are solicited to bid on this contract as prime contractors and are encouraged to make inquiries regarding potential subcontracting opportunities and equipment, material and/or supply needs.

MINIMUM WAGE RATES for this project have been predetermined by the Secretary of the Department of Labor in accordance with the requirements of the Federal regulations governing the expenditure of FEDERAL AID HIGHWAY FUNDS and are set out in the labor regulations contained in the proposal

All bidders must make positive efforts to use small and minority owned business and women business enterprises.

Bids may be submitted in a sealed envelope or electronically in “PDF” format.

Sealed bids shall be marked plainly on the exterior of the envelop:

5-LANE ROADWAY CONSTRUCTION OF I-10 CONNECTOR / MALLET ROAD

PROJECT NO. MS 134-030(2)B

and shall be addressed to the Clerk of the Board of Supervisors of Jackson County, 2915 Canty Street, Suite R, Pascagoula, MS 39567, prior to the hour and date designated above, and shall list the name and address of the company submitting the bid.

Bids submitted electronically shall contain the same information and forms as that required for the paper bid.

Bid documents may be viewed and/or downloaded at [www.neel-schafferplans.com](http://www.neel-schafferplans.com), or [www.jacksoncoplans.com](http://www.jacksoncoplans.com). A valid e-mail address is required for registration and log-in. Bid documents are nonrefundable and must be purchased through the website or ordered from Plan House. Electronic Bids shall be submitted to the Plan House website. For information regarding website registration, log-in purchase of bid documents, and Bid submission, please contact Plan House at (228) 248-0181.

The bid documents are on file and may be examined at the following locations:

1. Jackson County Road Department, 8500 Jim Ramsay Road, Vancleave, MS 39565
2. Neel-Shaffer, Inc., 707 Watts Ave., Suite C, Pascagoula, MS 39567
3. Mississippi procurement Technical Assistance Program (MPTAP)

Mississippi Development Authority, Minority & Small Business Development

Woolfolk Building, 501 North West Street, Suite B 01, Jackson, MS 39201

1. South MS Contract Procurement Center

1636 Popps Ferry Road, Suite 203, Biloxi, MS 39532

Phone (228) 396-1288

Certified check or bid bond in the amount of five percent (5%) of the total bid, made payable to Jackson County and the State of Mississippi must accompany each proposal. Bid Bonds shall be valid for a minimum of 90 days.

The attention of the BIDDER is directed to the Bidder’s Checklist in the front of the Contract Documents, which will assist the Contractor in the submission of a compete Bid Proposal.

The successful Bidder will be required to obtain a Certificate of Responsibility from the Mississippi State Board of Contractors prior to being awarded the Contract.

Bidders are hereby notified that any proposal accompanied by letters qualifying in any manner the condition under which the proposal is tendered will be considered an irregular bid and such proposal will not be considered in making the award.

Melton Harris, Jr., President

Jackson County Board of Supervisors