OFFICE OF STATE AID ROAD CONSTRUCTION

 MISSISSIPPI DEPARTMENT OF TRANSPORTATION

 AND

 STONE COUNTY BOARD OF SUPERVISORS

 SECTION 900

 \_\_\_\_\_\_\_\_\_\_\_

 NOTICE TO CONTRACTORS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Sealed bids will be received by the Board of Supervisors of Stone County,

 Mississippi at the Stone County Courthouse, Wiggins, Mississippi, until 10:00 am on

 the 16th day of March, 2020 and shortly thereafter publicly opened for the

 construction of 0.076 miles of BRIDGE REPLACEMENT & APPROACHES on the INDA ROAD EAST

 being known as Project No. ERBR-66(03) in Stone County, Mississippi.

 PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 ITEM QUANTITY UNIT

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 ROADWAY ITEMS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_

 MOBILIZATION LUMP SUM LS

 CLEARING AND GRUBBING LUMP SUM LS

 REMOVAL OF BRIDGE (STA. 10+78) 1.000 UN

 REMOVAL OF EXISTING PAVEMENT 804.000 SY

 BORROW EXCAVATION (F.M.E.) 945.000 CY

 (CONTRACTOR FURNISHED) (CLASS 9)

 GRANULAR MATERIAL (LVM) 448.000 CY

 (CLASS 6, GROUP C)

 CRUSHED STONE (SIZE 610) (LVM) 90.000 CY

 HOT MIX ASPHALT, ST, 9.5mm 82.000 TON

 HOT MIX ASPHALT, ST, 12.5mm 186.000 TON

 GUARD RAIL, BRIDGE END SECTION, 4.000 EA

 TYPE "I" THRIE BEAM

 GUARD RAIL, TERMINAL END SECTION 4.000 EA

 RIGHT-OF-WAY MARKERS (TYPE I) 10.000 EA

 MAINTENANCE OF TRAFFIC LUMP SUM LS

 ADDITIONAL CONSTRUCTION SIGNS 0.000 SF

 4" WIDE THERMOPLASTIC EDGE STRIPE 0.151 MI

 (CONTINUOUS WHITE) (60 MIL)

 4" WIDE THERMOPLASTIC TRAFFIC 800.000 LF

 STRIPE (CONTINUOUS YELLOW) (90 MIL)

 THERMOPLASTIC LEGEND 132.000 LF

 (WHITE) (120 MIL)

 THERMOPLASTIC LEGEND 63.000 SF

 (WHITE) (120 MIL)

 REFLECTORIZED TRAFFIC WARNING SIGN 1.000 EA

 (ENCAPSULATED LENS)

 REFLECTORIZED TRAFFIC OBJECT MARKER 4.000 EA

 (ENCAPSULATED LENS)(TYPE 3)

 REFLECTORIZED ADVANCED WARNING SIGN 1.000 EA

 (ENCAPSULATED LENS)

 REFLECTORIZED TRAFFIC REGULATORY 1.000 EA

 SIGN WITH SUPP. PLATE

 (ENCAPSULATED LENS)

 Page 1 of 3

================================================================================

 SECTION 900

 PROJECT NO. ERBR-66(03)

 STONE COUNTY

 컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴

 GEOTEXTILE UNDER CRUSHED STONE 152.000 SY

 (TYPE V) (AOS 0.21-0.43)

 EROSION CONTROL ITEMS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 SOLID SODDING 200.000 SY

 EXCELSIOR BLANKET 200.000 SY

 HYDROSEEDING 0.650 AC

 TEMPORARY SILT FENCE 937.000 LF

 (TYPE II) (AOS 0.15-0.84)

 LOOSE RIPRAP, 200 LB. 112.000 TON

 GEOTEXTILE UNDER RIPRAP 175.000 SY

 (TYPE V) (AOS 0.21-0.43)

 WATTLES, 20" 600.000 LF

 BRIDGE ITEMS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_

 TEST PILE 2.000 EA

 CONVENTIONAL STATIC PILE LOAD TEST 0.000 EA

 14" PRESTRESSED CONCRETE PILING 750.000 LF

 18" PRE-FORMED PILE HOLES 372.000 LF

 19' PRECAST CONCRETE SLAB UNIT, 12.000 EA

 3'-6" INTERIOR

 31' PRECAST CONCRETE SLAB UNIT, 6.000 EA

 3'-6" INTERIOR

 19' PRECAST CONCRETE SLAB UNIT, 4.000 EA

 3'-6" EXTERIOR

 31' PRECAST CONCRETE SLAB UNIT, 2.000 EA

 3'-6" EXTERIOR

 PRECAST CONCRETE BARRIER RAIL 138.000 LF

 31' PRECAST CONCRETE CAP, 2.000 EA

 INTERMEDIATE UNIT, CONCRETE PILE

 31' PRECAST CONCRETE CAP, 2.000 EA

 END UNIT, CONCRETE PILE

 9.25' PRECAST CONCRETE WING 4.000 EA

 LOOSE RIPRAP, 300 LB. 210.000 TON

 GEOTEXTILE UNDER RIPRAP 380.000 SY

 (TYPE V) (AOS 0.21-0.43)

 Page 2 of 3

================================================================================

 PROJECT NO. ERBR-66(03)

 STONE COUNTY

 NOTICE TO CONTRACTORS:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 CONTRACT TIME: 120 Working Days

 BASIS OF AWARD

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_

 The award, if made, will be made to the lowest qualified bidder on the basis of

 published quantities.

 The attention of the BIDDER is directed to the State and Federal laws governing

 selection of and employment of labor.

 MINIMUM WAGE RATES for this project have been predetermined by the Secretary of the

 the Department of Labor in accordance with the requirements of Federal regulations

 governing the expenditure of FEDERAL AID HIGHWAY FUNDS and are set out in the labor

 regulations contained in the proposal.

 The Board of Supervisors hereby notifies all bidders that it will affirmatively

 insure that in any contract entered into pursuant to this advertisement, minority

 business enterprise will be afforded full opportunity to submit bids in response to

 this invitation and will not be discriminated against on the grounds of race, color,

 or national origin in consideration for an award.

 PLANS AND SPECIFICATIONS are on file in the Office of the Chancery Clerk of Stone

 County, the County Engineer's office and the Office of the State Aid Engineer, 412

 E. Woodrow Wilson Avenue, Jackson, Mississippi. This project shall be constructed

 in acccordance with the latest edition of the Mississippi Standard Specifications

 for State Aid Road and Bridge Construction.

 PLANS AND PROPOSALS may be secured from Jonathan K. Bond, County Engineer for Stone

 County, Mississippi, P. O. Box 369, Wiggins. The Cost is fifty dollars ($50.00) for

 plans and fifty dollars ($50.00) for the proposal, non-refundable

 Certified check or bid bond for five percent (5%) of the total bid, made payable to

 Stone County and the State of Mississippi must accompany each proposal.

 Bidders are hereby notified that any proposal accompanied by letters qualifying in

 any manner the condition under which the proposal is tendered will be considered an

 irregular bid and such proposal will not be considered in making the award.

 Lance Pearson, President

 Stone County Board of Supervisors

 Page 3 of 3