Hyperion Specifications

* Overall dimensions – 57“L x 28“W x 56“H on lockable castor wheels for ease of mobility
* Operates on 110V/22A
* PLC controlled with interactive HMI display
* 1750 Watt heater
* 2 fans for recirculation
* 8 amalgam UVC germicidal lights in quartz sleeves (1200W total)
* 2 thermocouples to ensure temperature is achieved and maintained
* 2 safety door interlocks to prevent opening door in operation
* Adjustable storage racks
* 30 cubic feet insulated disinfection chamber
* 20 feet recoil extension cord
* Local and remote operating and monitoring capability
* Proven successful in eliminating bacteria and viruses
* No toxic byproducts from UVC lamps
* Electrical enclosure is UL508a certified