**Sig Sauer P320 Carry 9mm**

**L320CA-9-BSS (Carry)**

**Specs**

**CALIBER** 9mm Luger

**ACTION TYPE** Semi-Auto

**FRAME SIZE** Carry

**FRAME FINISH**  Stainless Steel

**FRAME MATERIAL** Stainless Steel

**SLIDE FINISH** Nitron

**SLIDE MATERIAL** Stainless Steel

**ACCESSORY RAIL** M1913

**TRIGGER** Striker

**TRIGGER PULL DA** 6.5 lb (29 N)

**TRIGGER PULL SA** N/A

**BARREL LENGTH** 3.9 in (99 mm) , 4.6 in (117 mm)

**OVERALL LENGTH** 7.2in (183mm) - 7.9in (200mm)

**OVERALL WIDTH**  1.3 in (33 mm)

**HEIGHT** 5.5 in (140 mm)

**WEIGHT** 26.5 oz (751 g)

**Sig Sauer P320 Subcompact 9mm**

**L320SC-9-BSS (sub compact)**

**Specs**

**CALIBER** 9mm Luger

**ACTION TYPE** Semi-Auto

**FRAME SIZE** Sub-Compact

**FRAME FINISH** Stainless Steel

**FRAME MATERIAL** Stainless Steel

**SLIDE FINISH** Nitron

**SLIDE MATERIAL** Stainless Steel

**ACCESSORY RAIL** M1913

**TRIGGER** Striker

**TRIGGER PULL DA** 6.5 lb (29 N)

**TRIGGER PULL SA** N/A

**BARREL LENGTH** 3.6 in (91 mm)

**OVERALL LENGTH** 6.7 in (170 mm)

**OVERALL WIDTH** 1.3 in (33 mm)

**HEIGHT** 4.7 in (119 mm)

**WEIGHT** 24.9 oz (706 g)

**Sig Sauer P320 X Five Full Size 9mm**

**Specs**

**CALIBER** 9mm Luger

**FRAME MATERIAL** Polymer

**SLIDE FINISH** Nitron

**SLIDE MATERIAL** Stainless Steel

**BARREL MATERIAL** Carbon Steel

**ACCESSORY RAIL** M1913

**Details**

The P320 X-Five 9mm incorporates all of the most important features to maximize accuracy, shootability and ergonomics while maintaining the modularity of the standard P320 platform. The X-Series grip module is exclusive to this line and features a deeper trigger guard undercut, a higher back strap and an extended beavertail to ensure a higher grip for better recoil management. It also comes standard with a removable grip weight for improved balance, as well as a removable magazine funnel and extended slide catch lever to facilitate faster reloads. Like all X-Series P320s, the X-Five has the straight trigger that breaks at 90 degrees for an even better feeling pull. The 5" bull barrel and lightened slide pair perfectly for match-grade accuracy and are equipped with Dawson Precision® Fiber Optic front and fully adjustable rear sights. Additionally, the rear sight plate can be easily removed as a unit and replaced with a ROMEO1 optic, which means every P320 X-Five pistol is optics-ready right out of the box. Each P320 X-Five includes four (4) 21rd steel magazines.

**Safariland Duty Gear Technical Specification Package Model 7360 / 7365**

 Safariland LLC 3120 East Mission Boulevard\* P.O. Box 51478\* Ontario, California 91761 U.S.A. Tel. (909) 923-7300 Fax (909) 923-7400 www.safariland.com

 **General Description**

The 7360/7365 is a Level III Retention TM Duty Holster for pistol handguns. The body is injection molded with a proprietary nylon called Safari Seven which is resilient to extreme temperatures and completely non-abrasive to the firearm. The raised stand-off surface in the interior of the holster create air space around the weapon allowing dirt and moisture to quickly clear any contact with the firearm. Designed for use on a Safariland Sam Browne 2.25” (58mm) or 2” (50mm) belt. Model 7365 has a 1.5” drop.

Product Function

Maintains handgun in a stable, tactically ready configuration. Utilizes locking push down thumb platform and rotating hood to reduce take away potential. Also includes an internal locking device that retains the weapon in all directions when the primary device is open. Very easy to re-holster and secure by rotating hood back over handgun with Self Locking Snap-Free operation. Holster uses tension device for handgun adjustment. The adjusting screw is accessed from the opening in the muzzle end of the holster. Belt loop uses new, UBL (Universal Belt Loop) friction style design. Optional Sentry locking device (6001) can be mounted to any SLS system. Sentry provides an additional level of security. To operate the Sentry slide button forward with thumb to engage, slide Sentry back to disengage. Incorporates internal notch to keep lock engaged or disengaged under normal use. Injection molded out of impact resistant nylon.

Construction Materials

The holster is injection molded with a proprietary nylon called Safari Seven. It is structurally sound from 300 degrees to minus 50 degrees Fahrenheit. This material is non-abrasive to the firearms finish and can be maintained with a scouring pad. Polyester elastomer injection molded “SLS” strap with corrosion resistant stainless steel hardware. Hi-Carbon tempered steel spring with corrosion resistant film protectant. Case hardened nylon screws and t-nuts are used as fastening devices. The hardware is coated in black oxide and is rust resistant. Must be able to withstand a minimum of 48 hours submerged in water and retain shape and function. Exterior material to pass minimum of 2000 cycles at 1000 gms on taber abrasion test with H18 wheels.

Available Finishes

Plain Black and Flat Dark Earth Brown

Available Belt Loops

Standard 2.25” (58mm) or 2” (50mm) Universal Belt Loop (UBL)

Manufacturing Process

The holster body is injection molded with a proprietary nylon called Safari Seven. It is then folded in half to form the holster. It is fastened using case hardened fasteners. The belt loop and SLS hood are then assembled onto the body using the same type of hardware. The sight channel is molded in; the belt loop is injection molded for body curvature.

Dimensions and Weights: 7360 for Sig Sauer P320

Imperial Metric

Weight: .59 lbs .27 gr.

Length: 8 ¼” 20.95 cm

Height: 3 ⅞ 9.84 cm

Width: 3 ¾” 9.53 cm

Patent Information

7360/7365 falls under Patents: U.S. Pat. 7,694,860 B2 and patent pending

Quality Control

ISO 9001 Societe Generale de Surveillance – ANSI RAB Registrar AQS Quality Procedure.

Insurance Coverage

Safariland is