SINGLE AXLE DUMP TRUCK

AND DUMP BODY

Engine: Minimum 345 HP, 1150lbs./feet Torque

Transmission: Minimum Allison 3000 RDS Automatic with PTO Provision

Frame: 11/32 x 3 ½ x 10 15/16, Chrome Steel Bumper w/ tow hooks, rear tow hooks, Air & Electrical hookups for trailer

Front Axle: Minimum 12,000-lbs., spring minimum 12,000-lbs. taper leak, from shock absorbers, automatic slack adjusters

Rear Axle: Minimum 23,000-lbs., suspension minimum 23,000-lbs.

Tires: Front Wheels 22.5 x 8.25 10 Hub Pilot, Tires front 11R22.5 14 Ply Radial Hwy

 Rear Wheels 16.5 x 7 Q+ Cast Spider, Tires rear 11R22.5 14 Ply Radial Hwy

Add Gauges: Low air pressure light and buzzer, fuel gauge, rear axle temperature gauge, oil temperature gauge, engine oil pressure, speedometer with odometer, tachometer with hour meter, dual horn, driver display, day time running lights

Cab Interior: Must have Back up Alarm, Adjusting Steering Column, Tilt and Telescope, Seats- Driver High Back Air Suspension, AC/ Heat, auto self- reset circuit breaker in dash, seat covers leather with in board seat armrest, wood grain dash, power window and locks

Cab Exterior: LH and RH Exterior Grab Handles, tinted two piece windshield, spot mirrors 8” convex LH & RH, amber lights, heated mirrors with lights

Fuel Tanks: Minimum LH 80 Gallon Aluminum, minimum DEF tank 6 Gallon

Paint: Cab white base, Chassis black

Warranty: Minimum 1 Year/ 100,000 Mile Base Warranty on Chassis

Body Type: Standard square dump

Quality Reference: Ox Bodies Maverick

Body Length: 11’ feet

Side height: 42”

Tailgate height: 48”

Yardage: 10-11 yards

Understructure: 2”x8”x3/16” tubing, long sills, 1”x3”x11ga cross members on 12” centers

Frontage: One piece- 10 gauge Hi Tensile steel

Sides: 10 gauge, high tensile steel with vertical side braces, dirt shedding angle on bottom rail ladders and steps at front of body; tarp tie down rail full length of body on both sides

Top Rail: 4”x4”x11 gauge Top Rail

Floor: One Piece, 3/16” plate Hi tensile steel 5” floor strips on each side of body forming a forty-five (45) degree radius for easier clean out

Tailgate: One piece 3/16” plate Hi tensile steel with one dirt shedding horizontal brace pneumatic Hi-Lift operational air release tailgate

Cab Shield: 24” cab shield made of minimum 10-gauge

Dump Apron: 8” ¼” plate dump apron welded to rear

Hoist/ Hydraulics: NTEA Class 70 HYVA brand Hoist, Rated at 32 ton, 3 stage cylinder, active stage sizes (inches; 5,4,3), 82 inch stroke, 2 year warranty, APSCO Brand cab control console, air pump, hot shift PTO for Allison trans, direct mount Metaris Hydraulics Pump(48 GPM @ 1800 RPM, 2000 PSI steel hydraulic tank enclosed in doghouse

Boards: 8” hardwood boards painted to match body

Paint: Body to be metal shot blasted/ chipped primed with Sherwin Williams high build epoxy primer painted with polyurethane topcoat

Lighting: Custom wiring harness, Federal Standard 108 ALL LED lights

Tarp: Mountain Tarp Brand Electric Tarp System with Mesh (or vinyl) tarp cover, 5 year warranty on motor

Additional: Pintle Hitch and chip spreader bar

Warranty: 1 year from date of service unless otherwise indicated

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Other:

* Must give estimated time of delivery.
* Cost must include delivery to one of the county barns.
* Included Buy Back Option for 3, 4 and 5 years

Name of Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address of Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contact Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Location of Service Center: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Seller: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature of Seller: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_