**ADVERTISEMENT FOR BIDS**

Notice is hereby given that ***reverse auction bids*** will be received by the Adams County Board of Supervisors for the purchase, from the lowest and best bidder(s), of the following item as needed, for the Adams County Road Department, of a Mini Hydraulic Excavator.

Reverse Auction Bids will be received until August 24, 2023, no later than 10:00 A. M., at the County Administration Building, 314 State Street, Natchez, Mississippi.

Please review the Adams County Board of Supervisors website for steps to handling your reverse auction bids at <https://www.adamscountyms.net/>

Bidders wanting to access the reverse auction via telephone will be able to do so by calling 601-304-8098 at 10:00 A.M. C.S.T.

Bids submitted with qualifications or exceptions will not be considered.

Final Bid pricing is to be firm and not subject to change during the period specified above.

The Board of Supervisors reserves the right to waiver informalities and to reject any and all bids.

DE’NEEN PRICE

PURCHASE CLERK

601-445-7941 or 601-597-3160

BRANDI LEWIS

CHANCERY CLERK

ADAMS COUNTY, MISSISSIPPI

--------------------------------------------------------------------------------------------

**PUBLICATION DATES:**

**August 2, 2023**

**August 9, 2023**

**Reverse Auction: August 24, 2023**

Mini Hydraulic Excavator

Adams County Road Department 2023

Engine: Minimum net horsepower 54.8

Engine MUST meet U.S. EPA Tier 4 Final

Swing System: Minimum swing speed 10 RPM’s

Must have automatic swing break, spring applied,

hydraulic release

Travel Speed: Minimum low 1.9 MPH

Minimum high 3.1 MPH

Hydraulic System: Auxiliary hydraulic lines

Pump flow minimum 35 gal/min

Digging force arm minimum 30.7 KN

Digging force bucket minimum 46.6 KN

Hydraulic thumb

Blade: Angle or Straight Blade

Minimum Width 7’5”

Minimum height 17”

Minimum dig depth 12”

Minimum lift height 14”

Digging: Minimum depth 15’1”

Minimum reach 21’8”

Bucket: 24 inch

Lift Capacities: Minimum end lift at 3.0M reach

Undercarriage: Rubber or Steel Tracks

Cab Interior: Warning horn, cab and boom lights, retractable seat belt, monitor system, indicator lights on all gauges, review mirror, windshield wipers, and air conditioning and heat

Fuel Tank: Minimum 35.7 gal

Warranty: Full machine warranty for the duration of the lease, including any and all travel time and millage

Buybacks: 36- and 48-months machine buybacks must be provided

Other:

* Bidder shall have a certified parts and service center located within 50 miles of Natchez, MS Adams County
* Must give estimate time of delivery. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
* Cost must include delivery to one of the county barns.

Name of Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address of Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Contact Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Location of Service Center: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name of Seller: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature of Seller: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_