**Warning Siren Specifications**

**All products shall be manufactured with American Made components.**

**Siren System Proposal: (Battery Backed)**

**Warning Siren System Shall Include:**

-127 dB(c), Omni-Directional Siren -Siren Pole Mounting Brackets with Bolts

-Motor Contactor in NEMA 3R Enclosure -4 Function, Wireless Siren Controllers

-Complete, Turn Key Installation including -On Site Testing and Training

45’, Class Il utility pole

Power Disconnect -7 Year Warranty on Siren Head

6 Optima 34U Gel Cell Batteries

Power Supplies, Rectifiers, Transformers

**Complete, Siren, Basic Warning System Installed (AC/DC Battery Backed)**

Omni-directional warning sirens with associated components.

 The sirens will provide maximum coverage to citizens, agricultural workers, and individuals traveling through the jurisdiction

Locations

1  Elliott FD1 on Murff Dr
2  Geeslin Corner FD2 on Hwy 7 N
3  Geeslin Corner FD3 on Strider Rd
4  Gillon Cir (behind the area of the stop sign)
5  Misterton Rd @ Providence
6  Sparta Rd @ the water tank

\*Installation Notes:

Excludes any wiring, or work off of the siren pole.

Price is based on all sirens being ready for installation at the same time.

If hard rock is encountered when drilling to set poles any special equipment or extra time will

be billed as extra and separate.

Locations to be readily accessible for pole setting equipment.

Any required permits or inspection costs will be the responsibility of the city or county.

Adequate AC power must be supplied to the siren pole.

Costs subject to change with changes in siren quantities or models.

Cost does not include installation of power meter at siren site. Electric company shall provide

and install appropriate meter should one be required.

Please contact Mrs. Treiba Rodger Grenada Civil Defense Director at (662) 226-1076 for any location questions.