

# INVITATION FOR BIDSOFFICE OF PROCUREMENT & CONTRACTS

## INSTRUCTIONS FOR BIDDERS

* 1. Sealed bids will be received in the Office of Procurement & Contracts, Mississippi State University, for the purchase of the items listed herein.
	2. All bids must be received in the Office of Procurement & Contracts on or before the bid opening time and date listed herein. Delivery of bids must be during normal working hours, 8:00 a.m. to 5:00 p.m. CST, except on weekends and holidays when no delivery is possible.
	3. Bidders shall submit their bids either electronically or in a sealed envelope. To submit electronically, follow the instructions below. Bids CANNOT be emailed.
		1. Sealed bids should include the bid number on the face of the envelope as well as the bidders’ name and address. Bids should be sent to: 245 Barr Avenue, 610 McArthur Hall, Mississippi State, MS 39762.
		2. At this time we only accept non-ITS bids electronically. For electronic submission of bids, go to:portal.magic.ms.gov.
		and use the RFX number on the next page as your reference number.
	4. All questions regarding this bid should be directed to the Office of Procurement & Contracts at 662-325-2550.

## TERMS AND CONDITIONS

* 1. All bids should be bid “FOB Destination”
	2. Bidders must comply with all rules, regulations, and statutes relating to purchasing in the State of Mississippi, in addition to the requirements on this form. General Bid Terms and Conditions can be found here: <https://www.procurement.msstate.edu/procurement/bids/Bid_General_Terms_May_2019_V2.pdf>
	3. Any contract resulting from this Invitation for Bid shall be in substantial compliance with Mississippi State University’s Standard Contract Addendum: <https://www.procurement.msstate.edu/contracts/standardaddendum.pdf>

### Bid Number/RFX Number: ****23-43/RFX #3160005792****Opening Date: ****April 19, 2023 @2:00 p.m.****Description: ****2023 Dump Truck****

#### Vendor Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Vendor Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Telephone Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Days the Offer is Firm: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Authorized Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Title: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

| **Item** | **Quantity** | **Description** | **Unit Price** | **Total Price** |
| --- | --- | --- | --- | --- |
| 1 | 1 | 2023 Dump Truck |  |  |

2023 year model dump truck with a 7/8 yard bed, see minimum specs below;

TRUCK MUST BE WHITE IN COLOR

 DIESEL ENGINE HORSE POWER 260

 DIESEL ENGINE TORGUE 650

GVWR 33,000 POUNDS

PAYLOAD CAPACITY 23,500 POUNDS

SINGLE REAR AXLE 23,000 POUNDS

AIR BRAKES WITH 2 TANKS

TILT AND TELESCOPING STEERING WHEEL

CIGAR LIGHTER/12VOLT POWER OUTLET

AM/FM RADIO

HEATER AND AIR CONDITIONER

TILTING FRONT END

DRIVER AND PASSENGER SEATING

AIR SUSPENSION CAB

TOW HOOKS ON THE FRONT

ALLISON MANUAL TRANSMISSION WITH PTO PROVISION

HAND CONTROL THROTTLE

11R22.5 TIRES WITH A LOAD RANGE OF G

30 TON PINTLE HITCH

GLAD HANDS ON REAR OF TRUCK

D- RINGS ON THE REAR OF TRUCK

7 PIN RV STYLE ELECTICAL HOOK UP

DUMP BED MUST BE AT LEAST 10 FOOT LONG

7/8 YARDS CAPACITY

85CC GEAR PUMP

PTO OVER HYDRAULICS

32 INCH MINIMUM SIDE WALLS WITH VERTICLE BRACING

3/16 STEEL FLOOR

FULL WIDTH CAB SHIELD

AIR OPERATED TAIL GATE

ELCTRIC/MANUAL TARP COVER FOR BED

DUMP BED CAN BE BLACK IN COLOR