OFFICE OF STATE AID ROAD CONSTRUCTION

MISSISSIPPI DEPARTMENT OF TRANSPORTATION

AND

GREENE COUNTY BOARD OF SUPERVISORS

SECTION 900

NOTICE TO CONTRACTORS:

Sealed bids will be received by the Board of Supervisors of Greene County, Mississippi at the Greene County Courthouse, Leakesville, Mississippi, until 10:00 am on the 30th day of January, 2024 and shortly thereafter publicly opened for the construction of 0.155 miles of BRIDGES AND APPROACHES on the SITE "A"-OLD AVERA ROAD & SITE "B"-BATTLE ROAD being known as Project No. LSBP-21(13) in Greene County, Mississippi.

PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

ITEM QUANTITY UNIT

ROADWAY ITEMS:

MOBILIZATION LUMP SUM LS

CLEARING AND GRUBBING LUMP SUM LS

REMOVAL OF BRIDGE AT STATION 10+75 1.000 UN

REMOVAL OF BRIDGE AT STATION 23+54 1.000 UN

REMOVAL OF RIPRAP 200.000 SY

UNCLASSIFIED EXCAVATION (FM) 670.000 CY

EXCESS EXCAVATION (FM) 585.000 CY

GRANULAR MATERIAL (LVM), 785.000 CY

CLASS 9, GROUP B)

CRUSHED STONE, 610 260.000 TON

RIGHT-OF-WAY MARKERS (TYPE I) 19.000 EA

MAINTENANCE OF TRAFFIC LUMP SUM LS

ADDITIONAL CONSTRUCTION SIGNS 0.000 SF

REFLECTORIZED TRAFFIC OBJECT MARKER 8.000 EA

ENCAPSULATED LENS)(TYPE 3)

EROSION CONTROL ITEMS:

AGRICULTURAL LIMESTONE 2.400 TON

COMMERCIAL FERTILIZER (13-13-13) 1.200 TON

SEEDING 1.200 AC

VEGETATIVE MATERIALS FOR MULCH 3.600 TON

SOLID SODDING 200.000 SY

TEMPORARY SILT FENCE 1,750.000 LF

TYPE II) (AOS 0.15-0.84)

WATTLES, 20" 300.000 LF

LOOSE RIPRAP, 200 LB. 100.000 TON

GEOTEXTILE UNDER BRIDGE ABUTMENT, 200.000 SY

NON-WOVEN, TYPE V, AOS 0.21-0.43

GEOTEXTILE UNDER RIPRAP NON-WOVEN, 200.000 SY

TYPE V, AOS 0.21-0.43

Page 1 of 4

SECTION 900

PROJECT NO. LSBP-21(13)

GREENE COUNTY

BRIDGE - SITE "A ITEMS:

TEST PILE 2.000 EA

CONVENTIONAL STATIC PILE LOAD TEST 0.000 EA

14" PRESTRESSED CONCRETE PILING 910.000 LF

18" PRE-FORMED PILE HOLES 180.000 LF

BRIDGE CONCRETE, CLASS "B" 5.320 CY

REINFORCEMENT 635.000 LB

19' PRECAST CONCRETE SLAB UNIT, 6.000 EA

3'6" INTERIOR

31' PRECAST CONCRETE SLAB UNIT, 18.000 EA

3'6" INTERIOR

19' PRECAST CONCRETE SLAB UNIT, 2.000 EA

CURB

31' PRECAST CONCRETE SLAB UNIT, 6.000 EA

CURB

BEAM TYPE RAILING WITH 224.000 LF

CONCRETE POSTS

29' PRECAST CONCRETE CAP, 2.000 EA

INTERMEDIATE UNIT, CONCRETE PILE,

29' PRECAST CONCRETE CAP, 2.000 EA

END UNIT, CONCRETE PILE,

7.5' PRECAST CONCRETE WING 4.000 EA

LOOSE RIPRAP, 300 LB. 443.000 TON

GEOTEXTILE UNDER RIPRAP, 1,038.000 SY

NON-WOVEN, TYPE V, AOS < 0.43

BRIDGE - SITE "B" ITEMS:

TEST PILE 2.000 EA

CONVENTIONAL STATIC PILE LOAD TEST 0.000 EA

14" PRESTRESSED CONCRETE PILING 590.000 LF

18" PRE-FORMED PILE HOLE 140.000 LF

31' PRECAST CONCRETE SLAB UNIT, 18.000 EA

3'-6' INTERIOR, 30 DEG SKEW,

LT FWD.

31' PRECAST CONCRETE SLAB UNIT, 6.000 EA

CURB, 30 DEG SKEW, LT FWD

BEAM TYPE RAILING WITH 186.000 LF

CONCRETE POSTS

33'6" PRECAST CONCRETE CAP, 2.000 EA

INTERMEDIATE UNIT, CONCRETE PILE,

30 DEG SKEW, LT FWD.

33'6" PRECAST CONCRETE CAP, 2.000 EA

END UNIT, CONCRETE PILE,

30 DEG SKEW, LT FWD.

Page 2 of 4

SECTION 900

PROJECT NO. LSBP-21(13)

GREENE COUNTY

9.33' PRECAST CONCRETE WING 4.000 EA

LOOSE RIPRAP, 300 LB. 259.000 TON

GEOTEXTILE UNDER RIPRAP, 622.000 SY

NON-WOVEN, TYPE V, AOS < 0.43

Page 3 of 4

PROJECT NO. LSBP-21(13)

GREENE COUNTY

NOTICE TO CONTRACTORS:

CONTRACT TIME: 80 Working Days

BASIS OF AWARD

The award, if made, will be made to the lowest qualified bidder on the basis of published quantities.

The Board of Supervisors hereby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprise will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color, or national origin in consideration for an award.

PLANS AND SPECIFICATIONS are on file in the Office of the Chancery Clerk of Greene County, the County Engineer's office and the Office of the State Aid Engineer, 412 E. Woodrow Wilson Avenue, Jackson, Mississippi. This project shall be constructed in accordance with the latest edition of the Mississippi Standard Specifications for State Aid Road and Bridge Construction.

Plans and specifications are being made available via paper or digital copy. Plan Holders are required to log-in or register for an account to view or order bid documents at www.twaplanroom.com. For questions regarding website registration and online orders, please contact Plan House at 601-336-6378. For questions related to the contract documents, please contact The Walker Associates at 601-583-2127. No partial sets of drawings or bid documents will be issued.

All Proposals shall be submitted on Bid Forms provided with the specifications. Bids may be submitted in person, or for those interested, bids can be electronically submitted at www.twaplanroom.com under the project page. No oral, telegraphic, telephonic, or e-mail proposals will be considered.

Certified check or bid bond for five percent (5%) of the total bid, made payable to Greene County and the State of Mississippi must accompany each proposal. Bids will be accepted only under the name of the Bidder to whom PLANS AND PROPOSALS have been issued by the County Engineer, and whose name appears on the official list of planholders maintained by the County Engineer.

Bidders are hereby notified that any proposal accompanied by letters qualifying in any manner the condition under which the proposal is tendered will be considered an irregular bid and such proposal will not be considered in making the award.

Wayne Barrow, President

Greene County Board of Supervisors

Publish Dates: December 7, 2023 and December 14, 2023

Page 4 of 4