# OFFICE OF STATE AID ROAD CONSTRUCTION MISSISSIPPI DEPARTMENT OF TRANSPORTATION

AND

# WALTHALL COUNTY BOARD OF SUPERVISORS

SECTION 900

NOTICE TO CONTRACTORS:

Sealed bids will be received by the Board of Supervisors of Walthall County, Mississippi at the Walthall County Courthouse, Tylertown, Mississippi, until 10:00 am on the 24th day of October, 2018 and shortly thereafter publicly opened for the construction of 0.054 miles of BRIDGE MAINTENANCE on the DARBUN CHINA GROVE ROAD being known as Project No. SAP-74(20)M in Walthall County, Mississippi.

# PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

|  |  |  |
| --- | --- | --- |
| ITEM | QUANTITY | UNIT |
| ROADWAY ITEMS: |  |  |
| MOBILIZATION | LUMP SUM | LS |
| CLEARING AND GRUBBING | LUMP SUM | LS |
| REMOVAL OF BRIDGE @ STATION | 1.000 | UN |
| 80+00.14 |  |  |
| UNCLASSIFIED EXCAVATION (FM) | 297.000 | CY |
| SURPLUS EXCAVATION (FM) | 220.000 | CY |
| GRANULAR MATERIAL (LVM}, | 570.000 | CY |
| (CLASS 6, GROUP C} |  |  |
| HOT MIX ASPHALT, ST, 9.5mm | 81.000 | TON |
| ASPHALT FOR PRIME COAT | 260.000 | GAL |
| GUARD RAIL, W BEAM | 175.000 | LF |
| GUARD RAIL, BRIDGE END SECTION, SPECIAL DESIGN | 4. 000 | EA |
| GUARD RAIL, TERMINAL END SECTION MAINTENANCE OF TRAFFIC  ADDITIONAL CONSTRUCTION SIGNS | 4.000  LUMP SUM  0.000 | EA LS SF |
| 4" WIDE THERMOPLASTIC EDGE STRIPE (CONTINUOUS WHITE} (60 MILS } | 0.152 | MI |
| 4" WIDE THERMOPLAST IC TRAFFIC STRIPE (CONTINUOUS YELLOW} | 800.000 | LF |
| (90 MILS} |  |  |
| TWO-WAY YELLOW REFLECTIVE HIGH PERFORMANCE RAISED MARKERS | 8.000 | EA |
| REFLECTORIZED TRAFFIC OBJECT MARKER (ENCAPSULATED LENS } (TYPE 3) | 4.000 | EA |
| EROSION CONTROL ITEMS: |  |  |
| COMMERCIAL FERTILIZER (13-13-13) | 0.750 | TON |
| SEEDING | 0.750 | AC |
| VEGETATIVE MATERIALS FOR MULCH | 1.500 | TON |
| SOLID SODDING | 50.000 | SY |
| TEMPORARY SILT FENCE | 800.000 | LF |

SECTION 900

PROJECT NO. SAP-74(20)M WALTHALL COUNTY

|  |  |  |
| --- | --- | --- |
| (TYPE II) (AOS 0.15-0.84) WATTLES, 20 INCH | 200.000 | LF |
| BRIDGE ITEMS: |  |  |
| TEST PILE | 2.000 | EA |
| CONVENTIONAL STATIC PILE LOAD TEST | 0.000 | EA |
| 14" PRESTRESSED CONCRETE PILING | 990.000 | LF |
| 19' PRECAST CONCRETE SLAB UNIT, | 1.000 | EA |
| 3'-6" INTERIOR |  |  |
| 31' PRECAST CONCRETE SLAB UNIT, | 6.000 | EA |
| 3'-6" INTERIOR |  |  |
| 19' PRECAST CONCRETE SLAB UNIT, | 1.000 | EA |
| CURB |  |  |
| 31' PRECAST CONCRETE SLAB UNIT, | 2.000 | EA |
| CURB |  |  |
| BEAM TYPE RAILING WITH | 81.000 | LF |
| CONCRETE POSTS |  |  |
| 29'-0" PRECAST CONCRETE CAP, | 4.000 | EA |
| INTERMEDIATE UNIT, CONCRETE PILE |  |  |
| 29'-0" PRECAST CONCRETE CAP, | 2.000 | EA |
| END UNIT, CONCRETE PILE |  |  |
| 7.5' PRECAST CONCRETE WING | 4.000 | EA |
| 19' PRECAST CONCRETE SLAB UNIT, | 24.000 | EA |
| 3'-6" INTERIOR (SALVAGE AND |  |  |
| REINSTALLATION) |  |  |
| 19' PRECAST CONCRETE SLAB UNIT, | 8.000 | EA |
| CURB (SALVAGE AND REINSTALLAT ION) |  |  |
| BEAM TYPE RAILING WITH | 152.000 | LF |
| CONCRETE POSTS (SALVAGE AND |  |  |
| REINSTALLATION) |  |  |
| LOOSE RIPRAP, 300 LB. | 221.000 | TON |
| GEOTEXTILE UNDER RIPRAP,  TYPE V, AOS 0.21-0.43 | 382.000 | SY |

## PROJECT NO. SAP-74 (20)M

WALTHALL COUNTY

NOTICE TO CONTRACTORS:

CONTRACT TIME: 60 Working Days BASIS OF AWARD

The award, if made, will be made to the lowest qualified bidder on the basis of published quantities.

The Board of Supervisors hereby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprise will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color, or national origin in consideration for an award.

PLANS AND SPECIFICATIONS are on file in the Office of the Chancery Clerk of Walthall County, the County Engineer's office and the Office of the State Aid Engineer, 412

E. Woodrow Wilson Avenue, Jackson, Mississippi. This project shall be constructed in accordance with the latest edition of the Mississippi Standard Specifications for State Aid Road and Bridge Construction.

PLANS AND PROPOSALS may be secured from Jeff J. Dungan, County Engineer for Walthall County, Mississippi, 1574 Highway 98 East, Columbia. The Cost is dollars ($50.00} for plans and dollars ($50.00} for the proposal, non-refundable

Certified check or bid bond for five percent (5%} of the total bid, made payable to Walthall County and the State of Mississippi must accompany each proposal.

Bidders are hereby notified that any proposal accompanied by letters qualifying in any manner the condition under which the proposal is tendered will be considered an irregular bid and such proposal will not be considered in making the award.

Larry Montgomery, President

Walthall County Board of Supervisors

Publish On:

Thursday, September 20, 2018

Thursday, September 27, 2018