ADDENDUM NO. 1

Issued June 28th, 2018

RE: Change to the technical specifications of the Network Video Recorder in the RFP for Neshoba County General Hospital and Nursing Home Surveillance Video Management System, Bid Number 8200-20180620124515

From: Neshoba County General Hospital, IT Department

 1001 Holland Ave

 Philadelphia, MS 39350

To: Prospective Bidders

This addendum serves as a change to the technical specifications of the Hybrid Network Video Recorder Hardware in the Request for Proposal, bid number 8200-20180620124515. Prospective bidders are to take the following in to account in rendering a proposal for this work.

**Change to section 5.3.1 Server Features. The paragraph currently reads:**

The server shall be in a rack-mount chassis and shall fit in an EIA-standard rack utilizing no more than two units rack space. The operating system shall be at least Microsoft Windows Server 2012. Server shall have front accessible, hot swappable hard-disk trays.

**Is amended to read:**

The video recorder shall be in a rack-mount chassis and shall fit in an EIA-standard rack utilizing no more than two units rack space. The Operating System shall be at least Microsoft Windows 10 or equivalent.

**Change to section 5.3.2 Server System Features. The paragraph currently reads:**

 The server shall meet or exceed the following system component specifications:

* Server shall have at least 32GB of DDR3 system memory
* Server shall provide between 2TB and 12TB RAID5 with hot spare for internal storage of video event data
* Server shall have four Gigabit network controller ports
* Server shall have an RS-232C serial port for communications with a pan, tilt, zoom camera
* Server shall have the ability to support analog and IP cameras

**Is amended to read:**

The video recorder shall meet or exceed the following system component specifications:

* Recorder shall have at least 4GB of system memory
* Recorder shall provide at least 1TB of internal storage of video event data
* Recorder shall have at least one Gigabit Network port
* Recorder shall have the ability to support analog and IP cameras

Clarification

The wrong technical specifications were used for the Hybrid Video Recorder Hardware. An addendum is needed to reflect the minimum specifications that work for all video recorder hardware needed for this proposal.

Acknowledgment

Each bidder shall acknowledge receipt of this Addendum No. 1 of Bid Number 8200-20180620124515, Surveillance Video Management System by his/her signature affixed hereto, and shall attach this addendum to the proposal submitted.

Certification by Bidder:

Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Title:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Company:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_