OFFICE OF STATE AID ROAD CONSTRUCTION

MISSISSIPPI DEPARTMENT OF TRANSPORTATION

AND

THE CITY OF VICKSBURG

SECTION 900

 NOTICE TO CONTRACTORS:

 Sealed bids will be received by the Mayor and Aldermen of The City of Vicksburg, Mississippi, until 9:00 a.m., local time, November 16, 2020 at the City Clerk’s Office and shortly thereafter publicly opened and read aloud by the Board of Mayor and Alderman of the City of Vicksburg, Mississippi in Board meeting at 10:00 a.m., local time, November 16, 2020 for the construction of 0.142 miles of BRIDGE REPLACEMENT on KEMP BOTTOM ROAD being known as Project No. ERBR-SA-75(A022)in Warren County, Mississippi.

Electronic bids can be submitted at [www.centralbidding.com](http://www.centralbidding.com). Official bid documents can be downloaded from Central Bidding. Interested contractors can register as a vendor for free at [www.centralbidding.com](http://www.centralbidding.com) and download plans for $49.99. Electronic bids are due at the same time and date as sealed bids. For any questions relating to the electronic bidding process, please call 225-810-4814.

**Bidders are cautioned that the City Clerk does not receive the daily U.S. Mail on or before 9:00 a.m. Bids will be time-stamped upon receipt according to City Clerk’s time clock.**

 PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

 ITEM QUANTITY UNIT\_\_\_\_\_\_\_

ROADWAY ITEMS:

MOBILIZATION LUMP SUM LS

CLEARING AND GRUBBING LUMP SUM LS

REMOVAL OF OBSTRUCTIONS LUMP SUM LS

REMOVE AND RESET FENCE 138.00 LF

REMOVAL OF ASPHALT (ALL DEPTHS) 766.37 SY

REMOVAL AND REPLACEMENT OF RIPRAP 596.80 SY

REMOVAL OF PIPE (ALL SIZES) 25.00 LF

UNCLASSIFIED EXCAVATION (PM) 411.00 CY

BORROW EXCAVATION (CONTRACTOR 112.00 CY

FURNISHED)(LVM)(CLASS 9)

CHANNEL EXCAVATION (PM) 23,765.00 CY

GEOTEXTILE FABRIC STABILIZATION (TYPE V) 1,469.14 SY

GRUANULAR MATERIAL (CLASS 5, GROUP C) 189.84 TON

CRUSHED STONE (SIZE 610) 2,318.33 TON

NO. III STABILIZER AGGREGATE (COARSE) 2,996.15 TON

HOT MIX ASPHALT BASE COURSE (BB-1) 225.90 TON

Page 1 of 5

SECTION 900

PROJECT NO. ERBR-SA-75(A022)

WARREN COUNTY\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

HOT BITUMINOUS PAVEMENT SURFACE 112.95 TON

COURSE (SC-1) (TYPE 8)

COLD MILLING OF BITUMINOUS PAVEMENT, 657.17 SY

ALL DEPTHS

BITUMINOUS TACK COAT 68.45 GAL

CLASS 'A' STRUCTURAL CONCRETE 155.56 SY

18" CORRUGATED POLYETHLENE PIPE 152.00 LF

GUARDRAIL, BRIDGE END SECTION, 4.00 EA

TYPE "I" THRIE BEAM

GUARDRAIL, TERMINAL END SECTION 4.00 EA

ROADWAY/BRIDGE CONSTRUCTION STAKING LUMP SUM LS

ADJUSTMENT OF DRAINAGE STRUCTURES 1.00 UN

MAINTENANCE OF TRAFFIC LUMP SUM LS

ADDITIONAL CONSTRUCTION SIGNS 0.00 SF

4" WIDE THERMOPLASTIC EDGE STRIPE 0.28 MILE

(CONTINUOUS WHITE) (60 MILS)

4" WIDE THERMOPLASTIC TRAFFIC STRIPE 0.28 MILE

(CONTINUOS YELLOW) (90 MILS)

TWO-WAY YELLOW REFLECTIVE HIGH 20.00 EA

PERFORMANCE RAISED MARKERS

REFLECTORIZED TRAFFIC REGULATORY 1.00 EA

SIGN (ENCAPSULATED LENS)

REFLECTORIZED TRAFFIC OBJECT MARKER 4.00 EA

(ENCAPSULATED LENS)(TYPE 3)

REFLECTORIZED TRAFFIC DELINEATOR 8.00 EA

SIGN (ENCAPSULATED LENS)

EROSION CONTROL ITEMS:

AGRICULTURAL LIMESTONE 3.13 TON

COMMERCIAL FERTILIZER (13-13-13) 1.56 TON

AMMONIUM NITRATE 0.16 TON

SEEDING 1.56 ACR

VEGETATIVE MATERIAL FOR MULCH 3.13 TON

TEMPORARY SILT FENCE (TYPE 1) 3,000.00 LF

(AOS 0.15-0.84)

TEMPORARY EROSION CHECKS 192.00 BALE

WATTLES, 20" 480.00 LF

Page 2 of 5

BRIDGE ITEMS:

TEST PILE 2.00 EA

18" STEEL PILING, WALL THICKNESS 0.5000" 1,440.00 LF

DRILLED SHAFT, 60" DIAMETER 320.00 LF

TEST SHAFT, 60" DIAMETER 1.00 EA

TRIAL SHAFT, 60" DIAMETER 80.00 LF

BRIDGE CONTRECTE, CLASS "AA" 516.50 CY

100' PRESTRESSED CONCRETE BEAM TYPIE IV 1,483.10 LF

REINFORCEMENT 101,551.00 LBS

CONCRETE RAILING, 32" 595.40 LF

CONCRETE RAILING, 33.5" 40.00 LF

LOOSE RIPRAP, 500 LB. 10,692.27 TON

GROUTED RIPRAP, 300 LB. 723.75 SY

Page 3 of 5

 PROJECT NO. ERBR-SA-75(A022)

 WARREN COUNTY

NOTICE TO CONTRACTORS:

CONTRACT TIME: 200 Working Days

BASIS OF AWARD

Bidders must be qualified under Mississippi State law and possess a Certificate of Responsibility issued by the Mississippi State Board of Public Contractors. Each bidder shall write his Certificate of Responsibility number on the outside of the sealed envelope containing his proposal. For bids less than $50,000, a Certificate of Responsibility number is not required. Bidder shall note on the outside of the envelope containing the bid that the “bid is less than $50,000, CR No. not required”.

The contract time for the work included in this contract is **Two Hundred (200) Working Days**. The Contract will be subject to liquidated damages in accordance with the latest edition of the Mississippi Standard Specifications for State Aid Road and Bridge Construction.

The award, if made, will be made to the lowest qualified bidder on the basis of published quantities.

The City of Vicksburg hereby notifies all bidders that it will affirmatively insure that in any contract entered into pursuant to this advertisement, minority business enterprise will be afforded full opportunity to submit bids in response to this invitation and will not be discriminated against on the grounds of race, color, or national origin in consideration for an award.

Plans, specifications, and contract documents are on file and open to public inspection at the office of the City Clerk of Vicksburg. One (1) copy of the Plans, Specifications, and Contract Documents may be procured upon payment of $100.00 (by cash or check made payable to Stantec Consulting Services, Inc.) from Stantec Consulting Services, Inc., 901 Jackson Street, Vicksburg, Mississippi 39180. The payment is non-refundable. This project shall be constructed in accordance with the latest edition of the Mississippi Standard Specifications for State Aid Road and Bridge Construction.

Each bidder must deposit with his proposal a Bid Bond or Certified Check in an amount equal to five percent (5%) of the total bid payable to The City of Vicksburg as bid security. The successful bidder shall furnish a Performance Bond and a Payment Bond each in the amount of 100% of the contract amount awarded.

Bidders shall also submit a current financial statement if requested by The City of Vicksburg.

 Page 4 of 5

Attorneys-in-fact who sign Bid Bonds or Payment Bonds and Performance Bonds must file with each bond a certified and effective dated copy of their power of attorney.

Proposals shall be submitted in whole, sealed and deposited, with The City of Vicksburg prior to the hour and date above designated.

Bidders are hereby notified that any proposal accompanied by letters qualifying in any manner the condition under which the proposal is tendered will be considered an irregular bid and such proposal will not be considered in making the award.

 \_/s/Walter W. Osborne, Jr.\_\_\_\_\_

 Walter W. Osborne, Jr.

 City of Vicksburg

Publication Dates:

October 18, 2020

October 23, 2020



 Page 5 of 5