OFFICE OF STATE AID ROAD CONSTRUCTION

MISSISSIPPI DEPARTMENT OF TRANSPORTATION

AND

STONE COUNTY BOARD OF SUPERVISORS

SECTION 900

\_\_\_\_\_\_\_\_\_\_\_

NOTICE TO CONTRACTORS:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sealed bids will be received by the Board of Supervisors of Stone County,

Mississippi at the Stone County Courthouse, Wiggins, Mississippi, until 10:00 am on

the 16th day of March, 2020 and shortly thereafter publicly opened for the

construction of 0.076 miles of BRIDGE REPLACEMENT & APPROACHES on the INDA ROAD EAST

being known as Project No. ERBR-66(03) in Stone County, Mississippi.

PRINCIPAL ITEMS OF WORK ARE APPROXIMATELY AS FOLLOWS:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ITEM QUANTITY UNIT

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ROADWAY ITEMS:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

MOBILIZATION LUMP SUM LS

CLEARING AND GRUBBING LUMP SUM LS

REMOVAL OF BRIDGE (STA. 10+78) 1.000 UN

REMOVAL OF EXISTING PAVEMENT 804.000 SY

BORROW EXCAVATION (F.M.E.) 945.000 CY

(CONTRACTOR FURNISHED) (CLASS 9)

GRANULAR MATERIAL (LVM) 448.000 CY

(CLASS 6, GROUP C)

CRUSHED STONE (SIZE 610) (LVM) 90.000 CY

HOT MIX ASPHALT, ST, 9.5mm 82.000 TON

HOT MIX ASPHALT, ST, 12.5mm 186.000 TON

GUARD RAIL, BRIDGE END SECTION, 4.000 EA

TYPE "I" THRIE BEAM

GUARD RAIL, TERMINAL END SECTION 4.000 EA

RIGHT-OF-WAY MARKERS (TYPE I) 10.000 EA

MAINTENANCE OF TRAFFIC LUMP SUM LS

ADDITIONAL CONSTRUCTION SIGNS 0.000 SF

4" WIDE THERMOPLASTIC EDGE STRIPE 0.151 MI

(CONTINUOUS WHITE) (60 MIL)

4" WIDE THERMOPLASTIC TRAFFIC 800.000 LF

STRIPE (CONTINUOUS YELLOW) (90 MIL)

THERMOPLASTIC LEGEND 132.000 LF

(WHITE) (120 MIL)

THERMOPLASTIC LEGEND 63.000 SF

(WHITE) (120 MIL)

REFLECTORIZED TRAFFIC WARNING SIGN 1.000 EA

(ENCAPSULATED LENS)

REFLECTORIZED TRAFFIC OBJECT MARKER 4.000 EA

(ENCAPSULATED LENS)(TYPE 3)

REFLECTORIZED ADVANCED WARNING SIGN 1.000 EA

(ENCAPSULATED LENS)

REFLECTORIZED TRAFFIC REGULATORY 1.000 EA

SIGN WITH SUPP. PLATE

(ENCAPSULATED LENS)

Page 1 of 3

================================================================================

SECTION 900

PROJECT NO. ERBR-66(03)

STONE COUNTY

컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴

GEOTEXTILE UNDER CRUSHED STONE 152.000 SY

(TYPE V) (AOS 0.21-0.43)

EROSION CONTROL ITEMS:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

SOLID SODDING 200.000 SY

EXCELSIOR BLANKET 200.000 SY

HYDROSEEDING 0.650 AC

TEMPORARY SILT FENCE 937.000 LF

(TYPE II) (AOS 0.15-0.84)

LOOSE RIPRAP, 200 LB. 112.000 TON

GEOTEXTILE UNDER RIPRAP 175.000 SY

(TYPE V) (AOS 0.21-0.43)

WATTLES, 20" 600.000 LF

BRIDGE ITEMS:

\_\_\_\_\_\_\_\_\_\_\_\_\_

TEST PILE 2.000 EA

CONVENTIONAL STATIC PILE LOAD TEST 0.000 EA

14" PRESTRESSED CONCRETE PILING 750.000 LF

18" PRE-FORMED PILE HOLES 372.000 LF

19' PRECAST CONCRETE SLAB UNIT, 12.000 EA

3'-6" INTERIOR

31' PRECAST CONCRETE SLAB UNIT, 6.000 EA

3'-6" INTERIOR

19' PRECAST CONCRETE SLAB UNIT, 4.000 EA

3'-6" EXTERIOR

31' PRECAST CONCRETE SLAB UNIT, 2.000 EA

3'-6" EXTERIOR

PRECAST CONCRETE BARRIER RAIL 138.000 LF

31' PRECAST CONCRETE CAP, 2.000 EA

INTERMEDIATE UNIT, CONCRETE PILE

31' PRECAST CONCRETE CAP, 2.000 EA

END UNIT, CONCRETE PILE

9.25' PRECAST CONCRETE WING 4.000 EA

LOOSE RIPRAP, 300 LB. 210.000 TON

GEOTEXTILE UNDER RIPRAP 380.000 SY

(TYPE V) (AOS 0.21-0.43)

Page 2 of 3

================================================================================

PROJECT NO. ERBR-66(03)

STONE COUNTY

NOTICE TO CONTRACTORS:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

CONTRACT TIME: 120 Working Days

BASIS OF AWARD

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The award, if made, will be made to the lowest qualified bidder on the basis of

published quantities.

The attention of the BIDDER is directed to the State and Federal laws governing

selection of and employment of labor.

MINIMUM WAGE RATES for this project have been predetermined by the Secretary of the

the Department of Labor in accordance with the requirements of Federal regulations

governing the expenditure of FEDERAL AID HIGHWAY FUNDS and are set out in the labor

regulations contained in the proposal.

The Board of Supervisors hereby notifies all bidders that it will affirmatively

insure that in any contract entered into pursuant to this advertisement, minority

business enterprise will be afforded full opportunity to submit bids in response to

this invitation and will not be discriminated against on the grounds of race, color,

or national origin in consideration for an award.

PLANS AND SPECIFICATIONS are on file in the Office of the Chancery Clerk of Stone

County, the County Engineer's office and the Office of the State Aid Engineer, 412

E. Woodrow Wilson Avenue, Jackson, Mississippi. This project shall be constructed

in acccordance with the latest edition of the Mississippi Standard Specifications

for State Aid Road and Bridge Construction.

PLANS AND PROPOSALS may be secured from Jonathan K. Bond, County Engineer for Stone

County, Mississippi, P. O. Box 369, Wiggins. The Cost is fifty dollars ($50.00) for

plans and fifty dollars ($50.00) for the proposal, non-refundable

Certified check or bid bond for five percent (5%) of the total bid, made payable to

Stone County and the State of Mississippi must accompany each proposal.

Bidders are hereby notified that any proposal accompanied by letters qualifying in

any manner the condition under which the proposal is tendered will be considered an

irregular bid and such proposal will not be considered in making the award.

Lance Pearson, President

Stone County Board of Supervisors

Page 3 of 3