# Mississippi State UniversityInvitation for Bid 23-15, Composite Ply CutterAddendum Two

# January 24, 2023

The following question was received pertaining to the above bid file. See answer below and bid accordingly. Acknowledge this addendum by writing the number and date of the addendum on the bid form.

1. Regarding section 3.3 Machine Requirements, paragraph 3; a. “The vacuum system shall be monitored, and loss of vacuum shall trigger a machine interlock.” b. Is this feature a requirement? Or can it be quoted as an option?

a) Vacuum system monitoring is a desired feature but is not required. The intent of the statement is to prevent the machine from movement (or at least alert the user) in the event an operator forgets to start the vacuum system prior to running the file.