**HOT AND COLD BITUMINOUS ASPHALT MIXTURES**

**PERIOD JULY 1, 2024 THROUGH DECEMBER 31, 2024**

**Our price for material produced in accordance with Mississippi Department of Transportation Specifications.Trucks at our plant located at \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ are as follows:**

**TACK**

**(1) CSS-1H @\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per gallon**

**HOT BITUMINOUS PAVEMENT SURFACE COURSE GRADATION SC-1:**

**(2) Type 8, Crushed Gravel, or @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**Combined with Limestone or Slag**

**907-403-A HOT MIX ASPHALT, ST: (SEE NOTE 2)**

**(3) 4.75 mm Mixture @ \_\_\_\_ per ton**

**(4) 9.5mm Mixture @\_\_\_\_ \_\_\_\_\_\_ per ton**

**(5) 12.5 mm Mixture @ \_\_\_\_ per ton**

**(6) 19 mm Mixture @ \_\_\_\_ per ton**

**(7) 25 mm Mixture @ \_\_\_\_ per ton**

**907-403-A HOT MIX ASPHALT, MT: (SEE NOTE 2)**

**(8) 4.75 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(9) 9.5 mm Mixture @ \_\_\_\_ per ton**

**(10) 12.5 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(11) 19 mm Mixture @ \_\_\_\_ per ton**

**(12) 25 mm Mixture @ \_\_\_\_ per ton**

**907-403-A HOT MIX ASPHALT, HT: (SEE NOTE 2)**

**(13) 4.75 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(14) 9.5 mm Mixture @ \_\_\_\_ per ton**

**(15) 12.5 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(16) 19 mm Mixture @ \_\_\_\_ per ton**

**(17) 25 mm Mixture @ \_\_\_\_ per ton**

**907-403-A HOT MIX ASPHALT, HT, POLYMER MODIFIED (PG 76-22): (SEE NOTE 2)**

**(18) 4.75 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(19) 9.5 mm Mixture @ \_\_\_\_ per ton**

**(20) 12.5 mm Mixture @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(21) 19 mm Mixture @ \_\_\_\_ per ton**

**CONTRACTORS HOT MIX ASPHALT SPECIFICATIONS (SEE NOTE 1 and 3)**

**(22) Hot Mix Asphalt @\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**ULTRA-THIN HOT MIX ASPHALT (SEE NOTE 1 and 3)**

**(23) Hot Mix Asphalt @\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**404-A PRE-APPROVED COMMERCIAL COLD BITUMINOUS MIXTURES**

**(24) Bagged form:\_\_\_\_\_\_\_\_\_\_\_\_\_ Manufactured by:\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Product Name**

**@\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(25) Bulk form:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Manufactured by:\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Product Name**

**@\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**404-A MDOT STANDARD COLD BITUMINOUS MIXTURE**

**(26) Gradation Type D @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(27) Gradation Type E @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(28) Gradation Type F @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**(29) Gradation Type G @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**CONTRACTOR'S COLD BITUMINOUS MIXTURE SPECIFICATIONS**

**(30) Cold Mix Asphalt @\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ per ton**

**CONTRACTOR WILL DELIVER ASPHALT MIXTURES TO ANY POINT IN THE STATE FOR \_\_\_\_\_\_\_\_\_\_\_\_ PER TON PER MILE, WITH \_\_\_\_\_\_\_\_\_\_\_\_\_ PER TON MINIMUM HAUL.**

**NOTE 1: ONE (1) COPY OF CONTRACTOR'S SPECIFICATIONS FOR EACH BID ITEM MUST ACCOMPANY BID PROPOSAL.**

**NOTE 2: A material adjustment will be applied to this item as provided in Subsection 109.07 of the 2017 Edition of the Mississippi Standard Specifications for Road and Bridge Construction. The supplier must furnish material conforming to an approved MDOT HMA mix design. The adjustment code for this item is (A1) as set forth in Subsection 109.07.**

**Note 3: A materials adjustment will be applied to the Contractors Hot Mix Asphalt (HMA) as provided in Subsection 109.07 of the 2017 Edition of the Mississippi Standard Specifications for Roads and Bridge Construction. The adjustment code for the Contractors HMA is (A1) as set forth in Subsection 109.07; except the theoretical gallons will not be based on the job mix formula, but will be based the assumption that the mix has 5.0% new asphalt in it.**

COMPANY: \_**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** NAME: **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**(Print or Type)**

ADDRESS: \_**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ S**IGNED BY: **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** TITLE: **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

PHONE :**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** DATE :**\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

FAX : **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

EMAIL :**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**