SPECIFICATIONS

The Mississippi Bureau of Narcotics (MBN) is accepting proposals for 115 Conducted Electrical Weapon weapons with accessories. The payments will be spread out over a two year period for the equipment, accessories. Detailed specifications are as follows:

1. Conducted Electrical Weapon Handle (Unit)
	1. Data download capabilities (event log, pulse log and engineering log) when connected to a personal computer
	2. A high efficiency flashlight
	3. Unit housing should be high impact material
	4. Law Enforcement models only, no consumer models
	5. Real-time clock with back-up battery
	6. Safety switch
	7. Onboard self-diagnostic and system status monitoring and reporting capabilities
	8. Water resistant to IEC specification
	9. Red class IIIA Laser (for target acquisition)
2. RIGHT-HAND HOLSTER FOR CONDUCTED ELECTRICAL WEAPON
3. SPARE CARTRIDGE BATTERY BACK
4. 25’ CARTRIDGE
5. 15’ STANDARD CARTRIDGE (TRAINING PURPOSES)
6. DATAPORT DOWNLOAD USB KIT FOR USE WITH ALL CEW’S (2 KITS)
7. PLEASE INCLUDE TECHNICAL SPECIFICATIONS SHEET WITH BID